1. What is the first step in figuring board feet?
   1. Convert all measurements to inches
   2. Multiply all numbers in the numerator
   3. Divide the numerator by 144
   4. Multiply the by number of boards
2. What is the second step in figuring board feet?
   1. Convert all measurements to inches
   2. Multiply all numbers in the numerator
   3. Divide the numerator by 144
   4. Multiply the by number of boards
3. What is the third step in figuring board feet?
   1. multiply all numbers in the numerator
   2. Convert all measurements to inches
   3. Multiply the by number of boards
   4. Divide the numerator by 144
4. How many board feet are in the following boards? 2" x 4" x 12'
   1. 16
   2. 8
   3. 1.33
   4. .66

a. alkyd-oil paint e. latex paint i. semi-gloss finish paint b. flat finish paint f. long-oil alkyd paint j. short-oil alkyd paint c. gloss finish paint g. medium-oil alkyd paint d. Kilz or Bin paint h. oil base paint

1. \_\_\_\_\_\_\_ Paint cleaned up with a petroleum-based solvent preferred by professional painters as an exterior primer paint.
2. \_\_\_\_\_\_\_ Paint that is fast drying, for a harder, more durable surface composed of an oil and alkyd resin.
3. \_\_\_\_\_\_\_ Paint commonly used as an appliance and automotive enamel.
4. \_\_\_\_\_\_\_ Paint that is a high quality interior paint or an exterior trim enamel with great elasticity and durability.
5. \_\_\_\_\_\_\_ Paint finish that is a high priced paint that is durable, washes well, and brings out all defects in the surface.
6. \_\_\_\_\_\_\_ Paint sold as porch and floor enamel.
7. \_\_\_\_\_\_\_ Paint preferred by homeowners partially because of easy clean-up with soap and water.
8. \_\_\_\_\_\_\_ Paint finish type that is usually used on interior walls.
9. \_\_\_\_\_\_\_ Paint finish that withstands wear, washes well, and is used in kitchens, bathrooms, and as a trim paint (where a flat paint was used).
10. \_\_\_\_\_\_\_ Paint that is used to block stains from showing through.